[version]
CatalogFile 			= w9xel90x.cat
signature			="$CHICAGO$"
Class				=Net
Compatible 			= 1
ClassGUID  			= {4D36E972-E325-11CE-BFC1-08002BE10318}
provider			=%V_MS%
DriverVer 			=8/02/2001,04.06.0001.0

[Manufacturer]
%V_3COM%=3COM

[SourceDisksNames]
50="ECD520P90X",,0  

[SourceDisksFiles]
El90xnd5.sys =50 
;El90xnd4.sys =50 
;el90xnd3.sys =50
w9xel90x.inf =50
;netdi90x.dll =50

[3COM]
%PCI\VEN_10b7&DEV_9050.DeviceDesc%=PCIEL905TX.ndi, PCI\VEN_10b7&DEV_9050 		
%PCI\VEN_10b7&DEV_9051.DeviceDesc%=PCIEL905T4.ndi, PCI\VEN_10b7&DEV_9051 	
%PCI\VEN_10b7&DEV_9000.DeviceDesc%=PCIEL900TPO.ndi, PCI\VEN_10b7&DEV_9000 		
%PCI\VEN_10b7&DEV_9001.DeviceDesc%=PCIEL900COMBO.ndi, PCI\VEN_10b7&DEV_9001





;*** WIN 9X EXLCUSIVE *************************************************************


[PCIEL905TX.ndi]
DriverVer	=8/02/2001,04.06.0001.0
AddReg		=PCIEL905TX.ndi.reg,EL90x.ndi.reg,802.1p_mode, EL90x.params.tx, Flow_Control, DriverInfoAddReg
CopyFiles	=EL90x.inf.CopyFiles, EL90x.ndis3.CopyFiles, EL90x.ndi.CopyFiles

[PCIEL905T4.ndi]
DriverVer	=8/02/2001,04.06.0001.0
AddReg		=PCIEL900COMBO.ndi.reg,EL90x.ndi.reg,802.1p_mode, EL90x.params.t4, Flow_Control, DriverInfoAddReg
CopyFiles	=EL90x.inf.CopyFiles, EL90x.ndis3.CopyFiles, EL90x.ndi.CopyFiles

[PCIEL900TPO.ndi]
DriverVer	=8/02/2001,04.06.0001.0
AddReg		=PCIEL900TPO.ndi.reg,EL90x.ndi.reg,802.1p_mode, EL90x.params.tp, Flow_Control, DriverInfoAddReg
CopyFiles	=EL90x.inf.CopyFiles, EL90x.ndis3.CopyFiles, EL90x.ndi.CopyFiles

[PCIEL900COMBO.ndi]
DriverVer	=8/02/2001,04.06.0001.0
AddReg		=PCIEL900COMBO.ndi.reg,EL90x.ndi.reg,802.1p_mode, EL90x.params.combo, Flow_Control, DriverInfoAddReg
CopyFiles	=EL90x.inf.CopyFiles, EL90x.ndis3.CopyFiles, EL90x.ndi.CopyFiles

;------------------------------------

[PCIEL900TPO.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_10b7&DEV_9000"

[PCIEL900COMBO.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_10b7&DEV_9001"

[PCIEL905TX.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_10b7&DEV_9050"

[PCIEL905T4.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_10b7&DEV_9051"

;------------------------------------

[EL90x.ndi.reg]
HKR,,DeviceVxDs,,El90xnd3.sys
HKR,,ProviderName,,%ProviderName%
HKR,Ndi,NdiInstaller,,"NETDI90X.DLL, MyNdiProc"
HKR,,DevLoader,,*ndis
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"
HKR,NDIS,LogDriverName,,"EL90xnd"
HKR,NDIS,MajorNdisVersion,1,00
HKR,NDIS,MinorNdisVersion,1,0A

HKR,NDIS\NDIS2,DriverName,,"EL90x$"
HKR,NDIS\ODI,DriverName,,"3C90x"
HKR,NDIS\ODI,FileName,,"3c90x.com"

HKR,Ndi\Interfaces,DefUpper,,"ndis2,ndis3,ndis4,ndis5"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis5,ndis4,ndis3,ndis2,odi"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"

HKR,Ndi\Install,ndis3,,"EL90x.ndis3"
HKR,Ndi\Install,ndis2,,"EL90x.ndis2"
HKR,Ndi\Install,odi,,"EL90x.odi"
HKR,,wakeonmagic,,"YES"
HKR,,wakeonlink,,"NO"

HKR,,NDIS_VERSION,,"AUTO"
HKR,NDI\params\NDIS_VERSION,,,"AUTO"
HKR,NDI\params\NDIS_VERSION,ParamDesc,,"NDIS Driver Version"
HKR,NDI\params\NDIS_VERSION,flag,1,20,00,00,00
HKR,NDI\params\NDIS_VERSION,optional,,0
HKR,NDI\params\NDIS_VERSION,type,,enum
HKR,Ndi\params\NDIS_VERSION\enum,AUTO,,"Auto Select"
HKR,Ndi\params\NDIS_VERSION\enum,NDIS4,,"NDIS 4"

HKR,,TCAUDIAG,,"TCAUM90X"
HKLM,Software\3Com\TCAUDIAG\TCAUM90X,DriverNames,,"3C90X.COM;EL90X.DOS;SYSTEM\EL90XND3.SYS;SYSTEM\EL90XND4.SYS;SYSTEM\EL90XND5.SYS"

;------------------------------------

[EL90x.inf.CopyFiles]
w9xel90x.inf

;------------------------------------

[EL90x.ndi.CopyFiles]
netdi90x.dll,,,2

;------------------------------------

[EL90x.odi]

;------------------------------------

[EL90x.odi.CopyFiles]
3c90x.com

;------------------------------------

[EL90x.ndis3]

;------------------------------------

[EL90x.ndis3.CopyFiles]
el90xnd5.sys,,,2
el90xnd4.sys,,,2
el90xnd3.sys,,,2

;------------------------------------

[EL90x.ndis2]

;------------------------------------

[EL90x.ndis2.CopyFiles]
EL90x.dos


;*** END WIN 9X EXCLUSIVE *********************************************************





;*** WIN 2K EXCLUSIVE *************************************************************

[PCIEL905TX.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 5
AddReg          = EL90x.reg.NT, EL90x.software.NT, 802.1p_mode.NT, Flow_Control.NT, EL90x.params.tx.NT, DriverInfoAddReg
CopyFiles       = EL90x.Driver.NT, EL90x.INFFile.NT

[PCIEL905TX.ndi.NT.Services]
AddService      = EL90x, 2, EL90x.Service.NT, EL90x.EventLog.NT

[PCIEL905T4.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 5
AddReg          = EL90x.reg.NT, EL90x.software.NT, 802.1p_mode.NT, Flow_Control.NT, EL90x.params.t4.NT, DriverInfoAddReg
CopyFiles       = EL90x.Driver.NT, EL90x.INFFile.NT

[PCIEL905T4.ndi.NT.Services]
AddService      = EL90x, 2, EL90x.Service.NT, EL90x.EventLog.NT, DriverInfoAddReg

[PCIEL900TPO.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 5
AddReg          = EL90x.reg.NT, EL90x.software.NT, 802.1p_mode.NT, Flow_Control.NT, EL90x.params.tp.NT, DriverInfoAddReg
CopyFiles       = EL90x.Driver.NT, EL90x.INFFile.NT

[PCIEL900TPO.ndi.NT.Services]
AddService      = EL90x, 2, EL90x.Service.NT, EL90x.EventLog.NT

[PCIEL900COMBO.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 5
AddReg          = EL90x.reg.NT, EL90x.software.NT, 802.1p_mode.NT, Flow_Control.NT, EL90x.params.combo.NT, DriverInfoAddReg
CopyFiles       = EL90x.Driver.NT, EL90x.INFFile.NT

[PCIEL900COMBO.ndi.NT.Services]
AddService      = EL90x, 2, EL90x.Service.NT, EL90x.EventLog.NT


;------------------------------------

[EL90x.Driver.NT]
el90xnd5.SYS,,,2

;------------------------------------

[EL90x.INFFile.NT]
w9xel90x.inf,,,2

;------------------------------------

[EL90x.reg.NT]
HKR, Ndi,               Service,    0, "EL90x"
HKR, Ndi\Interfaces,    UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,    LowerRange, 0, "ethernet"
HKR,, TCAUDIAG,,"TCAUM90X"

;------------------------------------

[EL90x.software.NT]
HKLM,Software\3Com\El90x\CurrentVersion,Description,0,"%ProductSoftwareDescription%"
HKLM,Software\3Com\El90x\CurrentVersion,MajorVersion,0x00010001,"%ProductMajorVersion%"
HKLM,Software\3Com\El90x\CurrentVersion,MinorVersion,0x00010001,"%ProductMinorVersion%"
HKLM,Software\3Com\El90x\CurrentVersion,Review,0x00010001,"%ProductReview%"
HKLM,Software\3Com\El90x\CurrentVersion,ServiceName,0,"%ProductSoftwareName%"
HKLM,Software\3Com\El90x\CurrentVersion,SoftwareType,0,"%SoftwareType%"
HKLM,Software\3Com\El90x\CurrentVersion,Title,0,"%ProductSoftwareTitle%"

HKLM,Software\3Com\El90x\CurrentVersion\NetRules,bindable,0x00010000,"%NetRuleSoftwareBindable%"
HKLM,Software\3Com\El90x\CurrentVersion\NetRules,bindform,0,"%NetRuleSoftwareBindForm%"
HKLM,Software\3Com\El90x\CurrentVersion\NetRules,class,0x00010000,"%NetRuleSoftwareClass%"
HKLM,Software\3Com\El90x\CurrentVersion\NetRules,type,0,"%NetRuleSoftwareType%"
HKLM,Software\3Com\El90x\CurrentVersion\NetRules,use,0,"%SoftwareType%"

;------------------------------------

[EL90x.Service.NT]
DisplayName     = %el90x.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\el90XND5.SYS
LoadOrderGroup  = NDIS

;------------------------------------

[EL90x.EventLog.NT]
AddReg = el90x.AddEventLog.reg.NT

;------------------------------------

[EL90x.AddEventLog.reg.NT]
HKR,, EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\drivers\el90Xnd5.sys"
HKR,, TypesSupported,   0x00010001, 7

;End Win 2k Exclusive----------------







[strings]
InstallDiag= 				"YES"
InstallShortcuts= 			"YES"
InstallInstaller= 			"NO"
V_MS=					"3Com"
V_3COM=					"3Com"


ProviderName=				"3Com Corporation"
DriverVersion=				"8/02/2001,04.06.0001.0"
DriverVersion9x=			"07/16/2001"

el90x.Service.DispName = 		"3Com 3C90X Family PCI EtherLink Adapter"

ProductSoftwareDescription = 		"3Com 3C90X Adapter Driver"
ProductSoftwareTitle = 			"3Com 3C90x Adapter Driver"
ProductMajorVersion = 			"1"
ProductMinorVersion = 			"0"
ProductSoftwareName = 			"El90x"
ProductReview = 			"1"
SoftwareType = 				"driver"
NetRuleSoftwareType = 			"El90xSys ndisDriver El90xDriver"
NetRuleSoftwareBindForm = 		"""El90xSys"" yes no container"
NetRuleSoftwareClass = 			"El90xDriver basic"
NetRuleSoftwareBindable = 		"El90xDriver El90xAdapter non exclusive 100"

DISABLE= 				"Disable"
ENABLE= 				"Enable"
enable_all_caps=			"ENABLE"
enum=					"enum"
auto_select=				"Auto Select"
8021p= 					"802.1p Support"
flow_control=				"Flow Control"
hardware_default=			"Hardware Default"
media_type= 				"Media Type"
media_default= 				"HardwareDefault"
media_auto= 				"AutoSelect"
media_100Full= 				"100 Mb, Full Duplex"
media_100Half=				"100 Mb, Half Duplex"
media_10Full= 				"10 Mb, Full Duplex"
media_10Half= 				"10 Mb, Half Duplex"
media_10Base2= 				"10BASE-2, Half Duplex"
media_10AUI=				"AUI, Half Duplex"

; Driver Information Entries
; These items will be set by IHV...
DriverMfgr="3Com"                                     ; IHV name
DriverVersionID="03.61.0050.0"                        ; The IHV driver version
 BaseDriverFileName="El90xnd5.sys"                    ; Key file for version
 BaseDriverFileVersion="03.61.0050.0"                 ; version of key file
; These items will be set by IHV and updated by OEM
DriverOEM="3Com"                                      ; name of the OEM
DriverFamily="NIC"                                    ; device family (NIC, Storage, Video...)
DriverProduct="???"                                   ; Specific Name of device (chipset, for example)
DriverDescription="Description - DriverInfo sample"   ; Description of device (product name, OS or system supported)
DriverOEMVersion="5.4.0.0"                            ; OEM-specified version

PCI\VEN_10b7&DEV_9050.DeviceDesc=	"3Com EtherLink 10/100 PCI NIC (3C905-TX)"
PCI\VEN_10b7&DEV_9051.DeviceDesc=	"3Com EtherLink 10/100 PCI T4 NIC (3C905-T4)"
PCI\VEN_10b7&DEV_9000.DeviceDesc=	"3Com EtherLink PCI TPO NIC (3C900-TPO)"
PCI\VEN_10b7&DEV_9001.DeviceDesc=	"3Com EtherLink PCI Combo  NIC (3C900-COMBO)"

;------------------------------------

[DestinationDirs]
DefaultDestDir =11 
El90x.Driver.NT = 12
El90x.INFFile.NT = 17
EL90x.ndis3.CopyFiles =11 
EL90x.ndis2.CopyFiles =26 
EL90x.odi.CopyFiles =26 
EL90x.inf.CopyFiles =17 
EL90x.ndi.CopyFiles =11

;------------------------------------


[Flow_Control]
HKR,,FLOWCONTROL,,"ENABLE"
HKR,Ndi\params\FLOWCONTROL,			ParamDesc,		, %flow_control%
HKR,NDI\params\FLOWCONTROL,			flag,			1,30,00,00,00
HKR,Ndi\params\FLOWCONTROL,			type,			, %enum%
HKR,Ndi\params\FLOWCONTROL,			default,		, %enable_all_caps%
HKR,Ndi\params\FLOWCONTROL\enum,		ENABLE,			, %ENABLE%
HKR,Ndi\params\FLOWCONTROL\enum,		DISABLE,		, %DISABLE%

[Flow_Control.NT]
HKR,,FLOWCONTROL,,"ENABLE"
HKR,Ndi\params\FLOWCONTROL,			ParamDesc,		, %flow_control%
HKR,Ndi\params\FLOWCONTROL,			type,			, %enum%
HKR,NDI\params\FLOWCONTROL,			optional,		, 0
HKR,Ndi\params\FLOWCONTROL,			default,		, %enable_all_caps%
HKR,Ndi\params\FLOWCONTROL\enum,		DISABLE,		, %DISABLE%
HKR,Ndi\params\FLOWCONTROL\enum,		ENABLE,			, %ENABLE%

[802.1p_mode]
HKR,,8021psupport,,%DISABLE%
HKR,NDI\params\8021psupport,,,%DISABLE%
HKR,Ndi\params\8021psupport,			ParamDesc,		, %8021p%
HKR,NDI\params\8021psupport,			flag,			1,20,00,00,00
HKR,Ndi\params\8021psupport,			type,			, %enum%
HKR,NDI\params\8021psupport,			optional,		, 0
HKR,Ndi\params\8021psupport\enum,		DISABLE,		, %DISABLE%
HKR,Ndi\params\8021psupport\enum,		ENABLE,			, %ENABLE%

[802.1p_mode.NT]
HKR,,8021psupport,,%DISABLE%
HKR,Ndi\params\8021psupport,			ParamDesc,		, %8021p%
HKR,Ndi\params\8021psupport,			type,			, %enum%
HKR,NDI\params\8021psupport,			optional,		, 0
HKR,Ndi\params\8021psupport,			default,		, %DISABLE%
HKR,Ndi\params\8021psupport\enum,		DISABLE,		, %DISABLE%
HKR,Ndi\params\8021psupport\enum,		ENABLE,			, %ENABLE%

[EL90x.params.tx]
HKR,,media_type,,%media_default%
HKR,NDI\params\media_type,,,%media_default%
HKR,NDI\params\media_type,			ParamDesc,		, %media_type%
HKR,NDI\params\media_type,			flag,			1,20,00,00,00
HKR,NDI\params\media_type,			type,			, %enum%
HKR,NDI\params\media_type,			optional,		, 0
HKR,Ndi\params\media_type\enum,			HARDWAREDEFAULT,	, %hardware_default%
HKR,Ndi\params\media_type\enum,			AUTO,			, %media_auto%
HKR,Ndi\params\media_type\enum,			10HALF,			, %media_10Half%
HKR,Ndi\params\media_type\enum,			10FULL,			, %media_10Full%
HKR,Ndi\params\media_type\enum,			100HALF,		, %media_100Half%
HKR,Ndi\params\media_type\enum,			100FULL,		, %media_100Full%

[EL90x.params.tx.NT]
HKR,,media_type,,%media_default%
HKR,Ndi\params\media_type,			ParamDesc,		, %media_type%
HKR,Ndi\params\media_type,			type,			, %enum%
HKR,Ndi\params\media_type,			optional,		, 0
HKR,Ndi\params\media_type,			default,		, %media_default%
HKR,Ndi\params\media_type\enum,			HARDWAREDEFAULT,	, %hardware_default%
HKR,Ndi\params\media_type\enum,			AUTO,			, %media_auto%
HKR,Ndi\params\media_type\enum,			10HALF,			, %media_10Half%
HKR,Ndi\params\media_type\enum,			10FULL,			, %media_10Full%
HKR,Ndi\params\media_type\enum,			100HALF,		, %media_100Half%
HKR,Ndi\params\media_type\enum,			100FULL,		, %media_100Full%


[EL90x.params.tp]
HKR,,media_type,,%media_default%
HKR,NDI\params\media_type,,,%media_default%
HKR,NDI\params\media_type,			ParamDesc,		, %media_type%
HKR,NDI\params\media_type,			flag,			1,20,00,00,00
HKR,NDI\params\media_type,			type,			, %enum%
HKR,NDI\params\media_type,			optional,		, 0
HKR,Ndi\params\media_type\enum,			HARDWAREDEFAULT,	, %hardware_default%
HKR,Ndi\params\media_type\enum,			AUTO,			, %media_auto%
HKR,Ndi\params\media_type\enum,			10HALF,			, %media_10Half%
HKR,Ndi\params\media_type\enum,			10FULL,			, %media_10Full%

[EL90x.params.tp.NT]
HKR,,media_type,,%media_default%
HKR,Ndi\params\media_type,			ParamDesc,		, %media_type%
HKR,Ndi\params\media_type,			type,			, %enum%
HKR,Ndi\params\media_type,			optional,		, 0
HKR,Ndi\params\media_type,			default,		, %media_default%
HKR,Ndi\params\media_type\enum,			HARDWAREDEFAULT,	, %hardware_default%
HKR,Ndi\params\media_type\enum,			AUTO,			, %media_auto%
HKR,Ndi\params\media_type\enum,			10HALF,			, %media_10Half%
HKR,Ndi\params\media_type\enum,			10FULL,			, %media_10Full%


[EL90x.params.t4]
HKR,,media_type,,%media_default%
HKR,NDI\params\media_type,,,%media_default%
HKR,NDI\params\media_type,			ParamDesc,		, "Network media Connection"
HKR,NDI\params\media_type,			flag,			1,20,00,00,00
HKR,NDI\params\media_type,			optional,		, 0
HKR,NDI\params\media_type,			type,			, %enum%
HKR,Ndi\params\media_type\enum,			HARDWAREDEFAULT,	, %hardware_default%
HKR,Ndi\params\media_type\enum,			AUTO,			, %auto_select%
HKR,Ndi\params\media_type\enum,			10HALF,			, %media_10Half%
HKR,Ndi\params\media_type\enum,			10FULL,			, %media_10Full%
HKR,Ndi\params\media_type\enum,			100HALF,		, %media_100Half%

[EL90x.params.T4.NT]
HKR,,media_type,,%media_default%
HKR,Ndi\params\media_type,			ParamDesc,		, %media_type%
HKR,Ndi\params\media_type,			type,			, %enum%
HKR,Ndi\params\media_type,			optional,		, 0
HKR,Ndi\params\media_type,			default,		, %media_default%
HKR,Ndi\params\media_type\enum,			HARDWAREDEFAULT,	, %hardware_default%
HKR,Ndi\params\media_type\enum,			AUTO,			, %media_auto%
HKR,Ndi\params\media_type\enum,			10HALF,			, %media_10Half%
HKR,Ndi\params\media_type\enum,			10FULL,			, %media_10Full%
HKR,Ndi\params\media_type\enum,			100HALF,		, %media_100Half%


[EL90x.params.combo]
HKR,,media_type,,%media_default%
HKR,NDI\params\media_type,,,%media_default%
HKR,NDI\params\media_type,			ParamDesc,		, %media_type%
HKR,NDI\params\media_type,			flag,			1,20,00,00,00
HKR,NDI\params\media_type,			type,			, %enum%
HKR,NDI\params\media_type,			optional,		, 0
HKR,Ndi\params\media_type\enum,			HARDWAREDEFAULT,	, %hardware_default%
HKR,Ndi\params\media_type\enum,			AUTO,			, %media_auto%
HKR,Ndi\params\media_type\enum,			10HALF,			, %media_10Half%
HKR,Ndi\params\media_type\enum,			10FULL,			, %media_10Full%
HKR,Ndi\params\media_type\enum,           	10BASE2,         	0, %media_10Base2%
HKR,Ndi\params\media_type\enum,           	10AUI,           	0, %media_10AUI%

[EL90x.params.combo.NT]
HKR,,media_type,,%media_default%
HKR,Ndi\params\media_type,			ParamDesc,		, %media_type%
HKR,Ndi\params\media_type,			type,			, %enum%
HKR,Ndi\params\media_type,			optional,		, 0
HKR,Ndi\params\media_type,			default,		, %media_default%
HKR,Ndi\params\media_type\enum,			HARDWAREDEFAULT,	, %hardware_default%
HKR,Ndi\params\media_type\enum,			AUTO,			, %media_auto%
HKR,Ndi\params\media_type\enum,			10HALF,			, %media_10Half%
HKR,Ndi\params\media_type\enum,			10FULL,			, %media_10Full%
HKR,Ndi\params\media_type\enum,         	10BASE2,         	0, %media_10Base2%
HKR,Ndi\params\media_type\enum,         	10AUI,           	0, %media_10AUI%

[DriverInfoAddReg]
; This section is added to all INFs to add registry entries for Driver Info.
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,Description,,%DriverDescription%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,CurrentVer,,%DriverOEMVersion%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,Ver_%DriverOEMVersion%,,%DriverVersionID%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%, BaseDriverFileName,,%BaseDriverFileName%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%, BaseDriverFileVersion,,%BaseDriverFileVersion%


;(%VER W9XEL90X.INF - Installation file for 905BC - v5.4.11)


