Start
Previous Next
7.1 The File Menu

### 7.1.29 Export/HPGL Plotter Output (only Windows)

Plot Vector Data prints the vector layers of a document to an HPGL-compatible plotter.

You can set the Port... (parallel, serial or file), to which the plotter is connected.

Plotting Speed defines, how fast the pen of the plotter is dragged on the paper or foil.

With border doesn’t draw the picture as small as possible, but uses the edge given by the picture.

If Only Selected is selected, only the active vector layer is drawn.

Offset allows you to enter a horizontal and vertical offset, so that you can plot several pictures side by side.

Paper Size should contain the size of the paper, so that PhotoLine can check, whether the picture fits on the page. Read From Plotter is working only, if the plotter is connected by a serial interface.

Picture Size defines the output size of the vector picture.