Start
Previous Next
7. The Menus / 7.4 The Layout Menu

### 7.4.78 Print Markers

Print Markers allows extended settings for printing, but which aren‘t necessary for standard printing.

Print Cut Markers shows additional strokes at the edge of the document to ease cutting the cutting by using a cutting machine. Because cutting often produces white lines at the edge, it is possible to move the stroke by using a text field.

If Print Registration Markers is turned on, at the 4 corners of the document small circles with a cross inside are printed. If you want to print your document in a print shop, those markers allow to place the four color channels of the document (usually cyan, magenta, yellow and black) exactly above each other.

Print Calibration Bar prints an additional color bar containing the color red, green, blue, cyan, magenta, yellow and black.

Print Densitometer Bar prints a color bar containing various densities for each basic print color.